# Mobile Capacity Inputs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **4G** | | | **5G** | | |
| **Parameter** | **Value** | **Source** | **Parameter** | **Value** | **Source** |
| Transmitter antenna type | Directional | [1] | Transmitter antenna type | Directional | [1] |
| Transmitter Power, Tx (dBm) | 43-46 | [2] | Transmitter Power, Tx dBm | 40 | [1] |
| Transmitter Antenna Gain (dBi) | 15-18 | [2] | Transmitter Antenna Gain (dBi) | 16 | [1] |
| Transmitter height (m) | 30 | [1] | Transmitter height (m) | 30 | [1] |
| UE antenna gain (dBi) | -5 - 10 | [2] | UE antenna gain (dBi) | 4 | [1] |
| UE antenna height (m) | 1.5 | [1] | UE antenna height (m) | 1.5 | [1] |
| Transmitter Feeder Loss (dB) | 2 | [3] | Transmitter Feeder Loss (dB) |  |  |
| Transmitter fade margin (dB) | 10 | [3] | Transmitter fade margin (dB) |  |  |
| UE losses (dB) | 4 |  | UE losses (dB) | 4 | [1] |
| UE fade margin (dB) | 0 | [3] | UE fade margin (dB) | 0 |  |
| Interference margin (dB) | 2 | [3] | Interference margin (dB) |  |  |
| UE noise figure (dB) | 8 | [3] | UE noise figure (dB) | 9 | [4] |
| Total sub-carriers | 512 | [3] | Total sub-carriers |  |  |
| Bandwidth (MHz) | 10 | [5] | Bandwidth (MHz) | 10 | [1] |
| Number of sectors | 3 | [6] | Number of sectors | 3 | [1] |
| Transmitting frequency (GHz) | 0.7, 1.8 | [5] | Transmitting frequency (GHz) | 0.7, 0.85 | [1] |
| Frequency reuse factor | 1 | [1] | Frequency reuse factor | 1 | [1] |
| Propagation model | HO | [7] | Propagation model | HO | [7] |
| System temperature (k) | 294 |  | System temperature (k) | 294 |  |
| Network load | 0.5, 0.6, 0.8 |  | Network load | 0.5, 0.6, 0.8 |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

Noise figure calculation: Evaluation of Radio Communication Links of 4G Systems

# Emissions Inputs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **4G** | | | **5G** | | |
| **Manufacturing Phase** | | | | | |
| **Parameter** | **Value** | **Source** | **Parameter** | **Value** | **Source** |
| BBU & RRU printed circuit board (kg) | 28.2 | [8] | BBU & RRU printed circuit board (kg) | 28.2 | [8] |
| BBU & RRU Aluminum (kg) | 112.8 | [8] | BBU & RRU Aluminium (kg) | 112.8 | [8] |
| Antenna system copper (kg) | 47.6 | [8] | Antenna system copper (kg) | 112.8 | [8] |
| Antenna system Aluminum (kg) | 19.7 | [8] | Antenna system Aluminium (kg) | 47.6 | [8] |
| Antenna system PVC (kg) | 6.8 | [8] | Antenna system PVC (kg) | 19.7 | [8] |
| Antenna system iron (kg) | 8.5 | [8] | Antenna system iron (kg) | 6.8 | [8] |
| Antenna system steel (kg) | 89.9 | [8] | Antenna system steel (kg) | 8.5 | [8] |
| Tower (kg) | 11,967.1 | [8] | Tower (kg) | 11,967.1 | [8] |
| Aluminium frame (kg) | 69 | [8] | Aluminium frame (kg) | 69 | [8] |
| Steel pole (kg) | 30.4 | [8] | Steel pole (kg) | 30.4 | [8] |
| Machine room concrete (kg) | 98,524.8 | [8] | Machine room concrete (kg) | 98,524.8 | [8] |
| Machine room steel (kg) | 895.7 | [8] | Machine room steel (kg) | 895.7 | [8] |
| Basic device Aluminum (kg) | 66.8 | [8] | Basic device Aluminum (kg) | 66.8 | [8] |
| **Transportation Phase** | | | | | |
| **Parameter** | **Value** | **Source** | **Parameter** | **Value** | **Source** |
| Vehicle emission factor (kg CO2 eq.) | 0.3234 |  | Vehicle emission factor (kg CO2 eq.) | 0.3234 |  |
| **Construction Phase** | | | | | |
| **Parameter** | **Value** | **Source** | **Parameter** | **Value** | **Source** |
| Machinery fuel efficiency (liters/hr) | 24.33 | [9] | Machinery fuel efficiency (liters/hr) | 24.33 | [9] |
| Machine operating hours (hours) |  |  | Machine operating hours (hours) |  |  |
| Diesel emission factor (kg CO2 eq.) | 2.68 | [10] | Diesel emission factor (kg CO2 eq.) | 2.68 | [10] |
| **Operations Phase** | | | | | |
| **Parameter** | **Value** | **Source** | **Parameter** | **Value** | **Source** |
| CPE power consumption (kWh) |  |  |  |  |  |
| Energy consumption (kWh) | 1.1 | [6] | Energy consumption (kWh) | 4.3 | [6] |
| Base band unit power, PBBU (W) | 89.377 | [6] | Base band unit power, PBBU (W) | 305.04 | [6] |
| Slope () | 6.6283 | [6] | Slope () | 1.6928 | [6] |
| Offset () | 156.6234 | [6] | Offset () | 389.7695 | [6] |
| Remote radio unit power, PRRU (W) | 288.8752 | [6] | Remote radio unit power, PRRU (W) | 406.6975 | [6] |
| Electricity emission factor (kg CO2 eq) | 0.1934 | [11] | Electricity emission factor (kg CO2 eq) | 0.1934 | [11] |
| **Material Carbon emission Factors (kg CO2 eq.)** | | | | | |
| **Material** | | | | **Value** | **Source** |
| Printed circuit board, (kg CO2 eq.) | | | | 29.76 | [6] |
| Aluminium, (kg CO2 eq.) | | | | 19.4 | [6] |
| Copper, (kg CO2 eq.) | | | | 4.91 | [6] |
| PVC, (kg CO2 eq.) | | | | 3.413 | [11] |
| Iron, (kg CO2 eq.) | | | | 2.14 | [6] |
| Steel, (kg CO2 eq.) | | | | 2.56 | [6] |
| Concrete, (kg CO2 eq.) | | | | 0.12 | [6] |
| **End of the Life Treatment, Open-Loop Recycling Carbon emission Factors (kg CO2 eq.)** | | | | | |
| **Material** | | | | **Value** | **Source** |
| Printed circuit board, (kg CO2 eq.) | | | | 21.28 | [6] |
| Aluminium, (kg CO2 eq.) | | | | 0.9847 | [6] |
| Copper, (kg CO2 eq.) | | | | 0.9847 | [6] |
| PVC, (kg CO2 eq.) | | | | 21.28 | [11] |
| Iron, (kg CO2 eq.) | | | | 0.9847 | [6] |
| Steel, (kg CO2 eq.) | | | | 0.9847 | [6] |
| Concrete, (kg CO2 eq.) | | | | 0.9847 | [6] |

Considering in Watts, the remote radio unit power (PRRU) is given by;

|  |  |
| --- | --- |
|  | (1) |

The

References